;
; Copyright 1999 - 2008 Microsoft Corporation


[Version]
Signature="$Windows NT$"
Provider=%MS%
LayoutFile=ntprint.inf
ClassGUID={4D36E979-E325-11CE-BFC1-08002BE10318}
Class=Printer
DriverVer=12/07/2010,1.0.0.1

;
; Manufacturer section.
;
; This section lists all of the manufacturers 
; that we will display in the Dialog box
;
[Manufacturer]
"YK"=T90, NTx86, NTamd64, NTia64
"YK"=T80, NTx86, NTamd64, NTia64
"YK"=POS58, NTx86, NTamd64, NTia64
"YK"=D5000, NTx86, NTamd64, NTia64
;
; Model sections. 
; 
; Each section here corresponds with an entry listed in the
; [Manufacturer] section, above. The models will be displayed in the order
; that they appear in the INF file.
;

[T90]
"T90 Driver"      =T90BITMAP

[T90.NTx86]
"T90 Driver"      = T90BITMAP

[T90.NTamd64]
"T90 Driver"      =T90BITMAP

[T90.NTia64]
"T90 Driver"      = T90BITMAP

[T80]
"T80 Driver"      =T80BITMAP

[T80.NTx86]
"T80 Driver"      = T80BITMAP

[T80.NTamd64]
"T80 Driver"      =T80BITMAP

[T80.NTia64]
"T80 Driver"      = T80BITMAP

[POS58]
"POS58 Driver"      =POS58BITMAP

[POS58.NTx86]
"POS58 Driver"      = POS58BITMAP

[POS58.NTamd64]
"POS58 Driver"      =POS58BITMAP

[POS58.NTia64]
"POS58 Driver"      = POS58BITMAP


[D5000]
"D5000 Driver"      =D5000BITMAP

[D5000.NTx86]
"D5000 Driver"      =D5000BITMAP

[D5000.NTamd64]
"D5000 Driver"      =D5000BITMAP

[D5000.NTia64]
"D5000 Driver"      = D5000BITMAP
;
; Installer Sections
;
; These sections control file installation, and reference all files that
; need to be copied. The section name will be assumed to be the driver
; file, unless there is an explicit DriverFile section listed.
;

[T90BITMAP]
CopyFiles=@T90.GPD
CopyFiles=@T90.INI
CopyFiles=T90BMP
DataFile=T90.GPD
DataSection=UNIDRV_DATA
Include=NTPRINT.INF
Needs=UNIDRV.OEM,UNIDRV_DATA

[T80BITMAP]
CopyFiles=@T80.GPD
CopyFiles=@T80.INI
CopyFiles=T80BMP
DataFile=T80.GPD
DataSection=UNIDRV_DATA
Include=NTPRINT.INF
Needs=UNIDRV.OEM,UNIDRV_DATA

[POS58BITMAP]
CopyFiles=@POS58.GPD
CopyFiles=@POS58.INI
CopyFiles=POS58BMP
DataFile=POS58.GPD
DataSection=UNIDRV_DATA
Include=NTPRINT.INF
Needs=UNIDRV.OEM,UNIDRV_DATA

[D5000BITMAP]
CopyFiles=@D5000.GPD
CopyFiles=@D5000.INI
CopyFiles=D5000BMP
DataFile=D5000.GPD
DataSection=UNIDRV_DATA
Include=NTPRINT.INF
Needs=UNIDRV.OEM,UNIDRV_DATA


; Copy Sections
;
; Lists of files that are actually copied. These sections are referenced
; from the installer sections, above. Only create a section if it contains
; two or more files (if we only copy a single file, identify it in the
; installer section, using the @filename notation) or if it's a color
; profile (since the DestinationDirs can only handle sections, and not
; individual files).
;

[T90BMP]
POS90D.DLL
POS90F.DLL
T90RES.dll
T90.GPD
T90.INI


[T80BMP]
POS80D.DLL
POS80F.DLL
T80RES.dll
T80.GPD
T80.INI

[POS58BMP]
POS58D.DLL
POS58F.DLL
POS58RES.dll
POS58.GPD
POS58.INI

[D5000BMP]
POS76D.DLL
POS76F.DLL
RES76.dll
D5000.GPD
D5000.INI


;
; Data Sections
;

; These sections contain data that is shared between devices.
;



;
;  Location of source files not in Layout.inf.
;

[SourceDisksNames]
100 = %OEMSample%

[SourceDisksFiles.x86]
pos90d.dll    = 100,T90\x86
pos90f.dll    = 100,T90\x86

pos80d.dll    = 100,T80\x86
pos80f.dll    = 100,T80\x86

pos58d.dll    = 100,POS58\x86
pos58f.dll    = 100,POS58\x86

pos76d.dll    = 100,D5000\x86
pos76f.dll    = 100,D5000\x86

[SourceDisksFiles.amd64]
pos90d.dll    = 100,T90\amd64
pos90f.dll    = 100,T90\amd64

pos80d.dll    = 100,T80\amd64
pos80f.dll    = 100,T80\amd64

pos58d.dll    = 100,POS58\amd64
pos58f.dll    = 100,POS58\amd64

pos76d.dll    = 100,D5000\amd64
pos76f.dll    = 100,D5000\amd64

[SourceDisksFiles.ia64]
pos90d.dll    = 100,T90\ia64
pos90f.dll    = 100,T90\ia64

pos80d.dll    = 100,T80\ia64
pos80f.dll    = 100,T80\ia64

pos58d.dll    = 100,POS58\ia64
pos58f.dll    = 100,POS58\ia64

pos76d.dll    = 100,D5000\ia64
pos76f.dll    = 100,D5000\ia64

[SourceDisksFiles]
T90.GPD       = 100
T90.INI    = 100

T80.GPD       = 100
T80.INI    = 100

POS58.GPD       = 100
POS58.INI    = 100

D5000.GPD       = 100
D5000.INI    = 100

;
; Call SetupSetDirectoryId with 66000 to set the target directory at runtime
; (depending on which environment drivers are getting installed)
;

[DestinationDirs]
DefaultDestDir=66000

;
; Localizable Strings
;
[Strings]
MS="YK"

